**SIEN HYDROLOGY LADWP GAGED STREAMS**

The City of Los Angeles Dept of Water and Power, LADWP, operates an extensive network of streamflow gaging stations along the east side slope of the Sierra Nevada as part of their Owens River project. The LADWP Hydrology Office in Bishop provided streamflow records for 5 gaging stations in response to a request for long-term records that represented essential unimpaired streamflows. These records are saved in the folder sien\_hydrology\_LADWP. Only monthly flows are available prior to the early 1990’s. The LADWP streamflow records for all 5 gages are shown on the first spreadsheet titled “LADWP”. Spreadsheets 2-6, identified by the stream name, show the information for each stream separately. The monthly mean discharge, Q, is given in cubic feet per second and the monthly volume of runoff is given in acre-feet.