The folder sien\_hydrology\_floods contains the annual series of instantaneous peak discharges recorded at each of the 22 USGS gaging stations considered to represent essentially unimpaired or natural conditions. The files were retrieved from the USGS California NWIS database located at <http://nwis.waterdata.usgs.gov/ca/nwis/peak>. The attached files were downloaded in the peakfq (watstore) format and have not been edited or modified. The attached files were used as input to the peakfq program (analysis of flood frequency) maintained and distributed by the USGS.